REQ\_001

The output fault shall be true when value differs from target.

REQ\_002

The output alarm shall be true when fault occurs during delay consecutives cycles.

REQ\_003

Once true, alarm shall be maintained until fault is false.